1. The adjustable flow stabilizer shall be a Singer Model 26 self-cleaning opening speed control, supplied as a stainless steel assembly.
2. The flow stabilizer shall allow unrestricted flow into the main valve bonnet while offering adjustable restricted flow out of the bonnet.
3. The Singer proprietary tapered internal orifice and inner valve shall offer precise adjustment, which shall be lockable by utilizing the top locknut.
4. The flow stabilizer shall improve low flow stability when incorporated with other “Singer Low Flow” proprietary automatic control valve enhancements