1. The non-modulating float control pilot shall be a Singer Model 43. The pilot shall be supplied with a *specify length 4 foot (1.2m), 6 foot (1.8m) or 10 foot (3.0m)* 316 stainless steel float rod and a 7” (178mm) diameter stainless steel float. The pilot body shall be of 316 stainless steel with Buna-N seals.
2. The pilot will close the main valve on rising water level (standard configuration).
3. Maximum working pressure: 80psi (5.5 bar)