1. The 82-PR adjustable pilot spring range shall be supplied with a spring range of *specify range (45 to 200psi, 7-25psi, 20-80psi or 100-300psi)*. The pilot shall be factory preset at *specify setpoint* psi.
2. The 82-PR pilot body shall be constructed of *specify material (ASTM B62 bronze or ASTM 316 stainless steel with a spring casing of specify material (ASTM B62 bronze or ASTM A351 CF8M stainless steel.*
3. The pilot elastomers: diaphragm, inner valve and seals, shall be of EPDM or Buna-N.
4. An adjustable needle valve closing speed control shall be supplied as *specify material ASTM B16 brass or AISI 316 stainless steel*.